Engine Oil Pan Removal

NOTE: Make sure to inspect the oil pump chain, when removing the oil pan. If the engine is out of the vehicle, go to Step 12 . Remove the splash shield. Drain the engine oil. Remove the drive belt. Remove the A/C compressor without disconnecting A/C line. Remove the lower torque rod (A), then remove the torque rod bracket (B). |

Remove the both subframe mid mounts mounting bolts. Remove the steering joint cover. Remove the steering gearbox from the subframe. |

Remove the subframe stiffener mounting bolts (A). Loosen the two subframe mounting bolts (B) so they are about 30 mm (1.2 in.) from the subframe. |

Remove the dipstick/tube (A) and O-ring (B). Remove the A/C compressor bracket. |

Remove the transmission mounting bolts. Remove the bolts securing the oil pan. |

Using a flat blade screwdriver, separate the oil pan from the block in the places shown. Inspect the oil pump chain. |