Combination Light Switch Test/Replacement

LHD type Remove the dashboard lower cover. Remove the steering column covers. Disconnect the 12P connector (A) from the wiper/washer switch (B). |

Remove the two screws, then slide out the combination light switch (A). |

1. Inspect the connector terminals to be sure they are all making good contact. If the terminals are bent, loose or corroded, repair them as necessary, and recheck the system. If the terminals look OK, check for continuity between the terminals in each switch position according to the tables.
   - | If there is no continuity replace switch.