Security Hood Switch Test

Open the hood. Disconnect the 2P connector from the hood switch. Check for continuity between the terminals. There should be continuity between the No. 1 and No. 2 terminals when the hood is opened (lever released). There should be no continuity between the No. 1 and No. 2 terminals when the hood is closed (lever pushed down). If the continuity is not as specified, replace the hood switch. |