Radiator

Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Radiator | Coolant capacities for K20A6 engine (including engine, heater, hoses, and reservoir) Use Genuine Honda All Season Antifreeze/Coolant Type 2 | M/T: engine overhaul | 6.6 L (1.74 US gal, 1.45 Imp gal)
M/T: coolant change | 4.5 L (1.19 US gal, 0.99 Imp gal)
A/T: engine overhaul | 6.5 L (1.72 US gal, 1.43 Imp gal)
A/T: coolant change | 4.4 L (1.16 US gal, 0.97 Imp gal)
Coolant capacities for K24A3 engine (including engine, heater, hoses, and reservoir) Use Genuine Honda All Season Antifreeze/Coolant Type 2 | M/T: engine overhaul | 7.4 L (1.95 US gal, 1.63 Imp gal)
M/T: coolant change | 5.4 L (1.43 US gal, 1.19 Imp gal)
A/T: engine overhaul | 7.3 L (1.93 US gal, 1.61 Imp gal)
A/T: coolant change | 5.3 L (1.40 US gal, 1.17 Imp gal)