LKAS Camera
DTC 7 and DTC 8: LKAS OFF indicator comes on in the MID
There was status that a vehicle was put on the environment that indoors becomes the high temperature (or the low temperature) which is extraordinary. It detects LKAS camera (at −10 °C/14 °F) low temperature (more than 60 °C/140 °F).
DTC 10: Adaptive cruise control (ACC)/LKAS indicator comes on
Static camera aiming failed with LKAS camera. Perform the camera aiming.
DTC 11: Adaptive cruise control (ACC)/LKAS indicator comes on
Dynamic camera aiming failed with LKAS camera. Perform the camera aiming.