SRS Side Curtain Airbag Replacement

Removal NOTE: Review the interior trim replacement procedure before performing repair or service Removal of the side curtain airbag must be performed according to the precautions/procedures described at the beginning of the SRS. The side curtain airbag system consists of the side curtain airbag module, including the roof trim and front grab handle. When the side curtain airbag has been deployed, these parts should be replaced. Disconnect the battery negative cable, and wait at least 3 minutes before beginning work. Remove the headliner trim. Disconnect the side curtain airbag subharness from the side curtain airbag 2P connector (A). |

Remove the mounting bolts (A) from the bracket. Remove the side curtain airbag assembly. |

Installation NOTE: Installation of the side curtain airbag must be performed according to the precautions/procedures described at the beginning of the SRS. If the airbag is frayed, or has only other visible damage, replace it. Do not attempt to repair an airbag. When you install the airbag, make sure it is not twisted, and not caught between the inflator bracket by the bracket bolts. Make sure that the side curtain airbag inflator retainer is installed properly, otherwise the airbag could accidentally deploy and cause damage or injuries. Place the new side curtain airbag assembly on the side of the roof. Tighten the side curtain airbag mounting bolts (A). |

Connect the side curtain airbag subharness from the side curtain airbag 2P connector (A). Reconnect the battery negative cable. After installing the side curtain airbag, confirm proper system operation: Turn the ignition switch ON (II); the SRS indicator should come on for about 6 seconds and then go off. Install all removed parts. |