Install the drive belt (A). Note these items during belt installation: Make sure that the belt is properly positioned on the pulleys (B). Do not get power steering fluid or grease on the auto-tensioner, alternator, A/C compressor, drive belt, or pulley faces. Clean off any fluid or grease before installation. Tighten the pump mounting bolts to the specified torque. Fill the reservoir to the upper level line. |