A/T End Cover Park Lever Stop Inspection and Adjustment

1. Set the park lever in the P position. Measure the distance (A) between the park pawl shaft (B) and the park lever roller pin (C).
   Standard: | 57.7−58.7 mm (2.27−2.31 in.)

If the measurement is out of standard, select and install the appropriate park lever stop (A) from the table. PARK LEVER STOP
Mark | Part Number | B | C
--- | --- | --- | ---
1 | 24537-PA9-003 | 11.00 mm (0.433 in.) | 11.00 mm (0.433 in.)
2 | 24538-PA9-003 | 10.80 mm (0.425 in.) | 10.65 mm (0.419 in.)
3 | 24539-PA9-003 | 10.60 mm (0.417 in.) | 10.30 mm (0.406 in.)
After replacing the park lever stop, make sure the distance is within tolerance. |