Measure the voltage between the No. 7 terminal of under-hood fuse/relay box connector E (16P) and body ground with the under-hood fuse/relay box connectors connected. Is there battery voltage?
YES | - | Repair open in the wire between the under-hood fuse/relay box and the fan control relay.■
NO | - | Repair open in the wire between the No. 30 fuse in the under-dash fuse/relay box and the under-hood fuse/relay box.■