1. Warm up the engine. Remove the maintenance lid (A). Remove the drain bolt (B), and drain the engine oil. Reinstall the drain bolt with a new washer (C). Refill with the recommended oil.
   Capacity
   At Oil Change:
   4.0 L (4.2 US qt, 3.5 Imp qt)
   At Oil Change including Filter:
   4.2 L (4.4 US qt, 3.7 Imp qt)
   After Engine Overhaul:
   5.3 L (5.6 US qt, 4.7 Imp qt)
Run the engine for more than 3 minutes, then check for oil leakage. |