Cut the lock tab (A) of the each shaft locknut (B) using a chisel (C). Then remove the locknuts and conical spring washers from each shaft. NOTE: Countershaft and secondary shaft locknuts have left-hand threads. Keep all of the chiseled particles out of the transmission. Clean the old mainshaft and countershaft locknuts; they are used to install the press fit idler gear on the mainshaft, and park gear on the countershaft. Remove the special tool from the mainshaft. |