1. SRS components are located in this area. Review the SRS component locations LHD, SRS component locations RHD and the precautions and procedures before performing repairs or service. NOTE: Put on gloves to protect your hands. Take care not to damage, wrinkle or twist the carpet. Be careful not to damage the dashboard or other interior trim pieces. If the side curtain airbag is equipped, disconnect the negative battery cable, and wait at least 3 minutes before beginning work. Remove these items: Front seats, both sides Rear seat cushion Rear seat side bolsters, both sides Kick panels, both sides Front door sill trim, both sides Rear door sill trim, both sides Center pillar lower trim
   - | Without side curtain airbag
   - | With side curtain airbag
Center console Driver's dashboard center lower cover Passenger's dashboard center lower cover Parking brake lever Stereo Amplifier Remove the front seat belt lower anchor bolt, both sides. Push the knob (A) back to release the hook (B) then pull up the accelerator pedal (C). |