1. Check Pull the parking brake lever (A) with 196 N (20 kgf, 44 lbf) of force to fully apply the parking brake. The parking brake lever should be locked within the specified number of clicks (B).
   Lever locked clicks: | 8 to 10
Adjust the parking brake if the lever clicks are not within the specification. NOTE: Minor parking brake lever adjustments (1 to 2 clicks) can be made with the adjusting nut in the equalizer. If a larger adjustment is required, follow the major adjustment procedure using the adjuster at the parking brake drum. After installing new parking brake shoes and/or new rear brake disc/drums, make sure you drive the vehicle for ‘‘break-in''. |