Cam Chain Auto-Tensioner Removal/Installation

Removal Remove the chain case cover. |

Turn the crankshaft counterclockwise to compress the auto-tensioner. |

Align the holes on the lock (A) and the auto-tensioner (B), then insert a 1.2 mm (0.05 in.) diameter pin or lock pin (P/N 14511-PNA-003) (C) into the holes. Turn the crankshaft clockwise to secure the pin. |

Remove the auto-tensioner. |

Installation Install the auto-tensioner. |

Remove the pin or lock pin (P/N 14511-PNA-003) from the auto-tensioner. Remove all of the old liquid gasket from the chain case cover mating surfaces, bolts, and bolt holes. Clean and dry the chain case cover mating surfaces. |

Apply liquid gasket, P/N 08C70-K0234M, 08C70-K0334M, or 08C70-X0331S, evenly to the chain case mating surface of the chain case cover and to the inner threads of the holes. NOTE: Do not install the parts if 4 minutes or more have elapsed since applying liquid gasket. Instead, reapply liquid gasket after removing old residue. |

Install the chain case cover. NOTE: Wait at least 30 minutes before filling the engine with oil. Do not run the engine within 3 hours after installing the chain case. |