Cylinder Head Rocker Arm Assembly Removal

Remove the cam chain. Loosen the rocker arm adjusting screws (A). |

Remove the camshaft holder bolts. To prevent damaging the camshafts, unscrew the bolts two turns at a time, in a crisscross pattern. Remove the cam chain guide B, camshaft holders, and camshafts. |

Insert the bolts (A) into the rocker shaft holder, then remove the rocker arm assembly (B). |