Special Tools Required Ball joint remover, 28 mm 07MAC-SL00201 or 07MAC-SL00200 Raise the front of the vehicle, and support it with safety stands in the proper locations. Remove the front wheel. Remove the damper fork (A) from the damper (B) and lower arm (C). NOTE: During installation, insert the damper fork into the damper lower end so the aligning tab (D) is aligned with the slot (E) in the damper fork. Replace the damper fork mounting nut (F) with a new one. |