Radiator

Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Radiator | Coolant capacities (including engine, heater, hoses, and reservoir) Use genuine Honda All Season Antifreeze/Coolant Type 2 (K20Z2) | M/T: engine overhaul | 6.7 L (1.77 US gal, 1.47 Imp gal)
M/T: coolant change | 4.8 L (1.27 US gal, 1.06 Imp gal)
A/T: engine overhaul | 6.6 L (1.74 US gal, 1.45 Imp gal)
A/T: coolant change | 4.7 L (1.24 US gal, 1.03 Imp gal)
Coolant capacities (including engine, heater, hoses, and reservoir) Use genuine Honda All Season Antifreeze/Coolant Type 2 (K24A3) | M/T: engine overhaul | 7.4 L (1.96 US gal, 1.63 Imp gal)
M/T: coolant change | 5.5 L (1.45 US gal, 1.21 Imp gal)
A/T: engine overhaul | 7.3 L (1.93 US gal, 1.61 Imp gal)
A/T: coolant change | 5.4 L (1.43 US gal, 1.19 Imp gal)