Remove the reservoir mounting bolt (A). Remove the clutch master cylinder (B), then remove the retaining clip (C) and clutch pipe (D). Plug the end of the clutch pipe with a shop towel to prevent brake fluid from coming out. Remove the O-ring (E) and clutch master cylinder seal (F) from the clutch master cylinder. Install the clutch master cylinder in the reverse order of removal, and note these items. When installing the clutch pipe to the clutch master cylinder, apply 0.05−0.1 g (0.0018−0.0035 oz) of the brake assembly lube on the mating surface. Tighten the master cylinder mounting nuts to 13 N·m (1.3 kgf·m, 9.4 lbf·ft). Install the air cleaner housing. Reconnect the battery cables; positive (+) cable first, then the negative (−) cable. Enter the anti-theft codes for the radio and the navigation system, then enter the customer's radio station presets. Perform the power window control unit reset procedure. |