DTC 86-1x (86-10 to 86-19, 86-1A to 86-1F): Faulty OPDS Seat-back Sensor DTC 86-2x (86-20 to 86-29, 86-2A to 86-2F): Faulty OPDS Seat Support Sensor Erase the DTC memory. Turn the ignition switch ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off. Does the SRS indicator stay on?
YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures.
NOTE: Aftermarket devices (fluorescent lights, laptop computers, etc.) used near the front passenger's seat-back can interfere with the seat-back sensors and cause a false DTC 86-1x or 86-2x. If one of these devices was used, erase the DTC, operate the device near the seat-back, and recheck for DTCs. If DTC 86-1x or 86-2x is reset, erase it, and do not use the device near the seat-back. Check the connection at the OPDS sensor harness connector and the OPDS unit connector. Are the connections OK?
YES | - | Go to Step 4 .
NO | - | Reconnect the OPDS sensor harness connector, and clear the DTC.■
Replace the OPDS sensor/seat-back foam , and initialize the OPDS. Erase the DTC memory, then check for DTC 86-1x or 86-2x. Is DTC 86-1x or 86-2x indicated?
YES | - | Replace the OPDS unit. ■
NO | - | The system is OK.■