DTC Troubleshooting: 107, 108

DTC 107: TCS Operation DTC 108: VSA Operation NOTE: The ABS/VSA indicators do not come on by memorizing the DTC 107 or 108. Clear the DTC using the HDS. Disconnect the HDS from the 16P DLC. Turn the ignition switch OFF, then turn it ON (II) again. Test-drive the vehicle. Is DTC 107 or DTC 108 indicated ?
YES | - | Check for loose terminals in the VSA control unit 47P connector. If necessary, substitute a known-good VSA modulator-control unit, and recheck.■
NO | - | Intermittent failure; the system is OK at this time.■