Resonator Removal/Installation

Make sure you have the anti-theft codes for the radio, then write down the frequencies for the radio's preset buttons. Remove the battery. Remove the intake air cover (A). Remove the bolts (B), and the resonator (C). Install the parts in the reverse order of removal. Reconnect the negative cable to the battery and do the following items: Power window control unit reset procedure. Enter the anti-theft codes for the radio and the navigation system, then enter the customer's radio station presets. Reset the clock. |