1. Displaying Sensor Inputs at the Climate Control Unit The climate control unit has a mode that displays sensor inputs it receives. This mode shows you what the climate control unit is receiving from each of the sensors, one at a time, and it can help you determine if a sensor is faulty. Check these items before using the sensor input display mode: Turn the ignition switch ON (II), and check the recirculation door function; press the recirculation button to switch from FRESH to RECIRC. The air volume and sound should change slightly. Set the temperature control knob to the desired test temperature. When selecting the test temperatures, note these items: ‘‘Lo'' temperature setting will default to MAX COOL, VENT, and RECIRC. ‘‘Hi'' temperature setting will default to MAX HOT, FLOOR, and FRESH. 16 through 28 °C settings will use the automatic climate control logic. Turn the ignition switch OFF. To run the sensor input display mode, follow these steps: Turn the ignition switch OFF. Press and hold both the AUTO and DUAL buttons, then start the engine. After the engine starts, release the buttons. The audio-HVAC display module display will flash the sensor number and then the value for that sensor. Record the valve displayed. To advance to the next sensor, press the rear window defogger button.
   Sensor | Item | Displayed Value
   --- | --- | ---
   1 | In-car Temperature Sensor | °C
   2 | Ambient Temperature | °C
   3 | Solar Radiation Sensor Value: Dark = 00, Flashlight = 04, Cloudy = 10, Sunny = 65 | kcal/m2·h
   4 | Engine Coolant Temperature | °C
   5 | Evaporator Outlet Air Temperature | °C
   6 | Driver's Air Mix Opening (Low value indicates cooler air distribution, higher value indicates warmer air distribution.) | % of opening
   7 | Passenger's Air Mix Opening (Low value indicates cooler air distribution, higher value indicates warmer air distribution.) | % of opening
   8 | Vehicle Speed (Vehicle must be driven to display speed) | km/h
   9 | Vent Temperature Air Out (TAO) | °C
   10 | A/C Pressure Sensor | MPa
1. NOTE: The sensor values will be displayed in degrees Celsius (°C) or an alphanumeric code. Use the chart to convert the value to degrees Fahrenheit (°F). If the sensor value displays ‘‘Er'' this indicates there is an open or short in the circuit or sensor. Check for DTCs using the HDS, or refer to checking DTCs by DTC indication to check for DTCs. If necessary, compare the sensor input display to an alike, known-good vehicle under the same test conditions. If the sensor is out of the normal range, refer to the sensor test, or substitute the sensor with a known-good, and recheck. To cancel the sensor input display mode, press the AUTO button, or turn the ignition off. Celsius to Fahrenheit Conversion Table
   °C | °F | °C | °F | °C | °F | °C | °F | °C | °F
   --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
   0 | 32 | 10 | 50 | 20 | 68 | 30 | 86 | 40 | 104
   1 | 34 | 11 | 52 | 21 | 70 | 31 | 88 | 41 | 106
   2 | 36 | 12 | 54 | 22 | 72 | 32 | 90 | 42 | 108
   3 | 37 | 13 | 55 | 23 | 73 | 33 | 91 | 43 | 109
   4 | 39 | 14 | 57 | 24 | 75 | 34 | 93 | 44 | 111
   5 | 41 | 15 | 59 | 25 | 77 | 35 | 95 | 45 | 113
   6 | 43 | 16 | 61 | 26 | 79 | 36 | 97 | 46 | 115
   7 | 45 | 17 | 63 | 27 | 81 | 37 | 99 | 47 | 117
   8 | 46 | 18 | 64 | 28 | 82 | 38 | 100 | 48 | 118
   9 | 48 | 19 | 66 | 29 | 84 | 39 | 102 | 49 | 120
   50 | 122 | 60 | 140 | 70 | 158 | 80 | 176 | 90 | 194
   51 | 124 | 61 | 142 | 71 | 160 | 81 | 178 | 91 | 196
   52 | 126 | 62 | 144 | 72 | 162 | 82 | 180 | 92 | 198
   53 | 127 | 63 | 145 | 73 | 163 | 83 | 181 | 93 | 199
   54 | 128 | 64 | 147 | 74 | 165 | 84 | 183 | 94 | 201
   55 | 131 | 65 | 149 | 75 | 167 | 85 | 185 | 95 | 203
   56 | 133 | 66 | 151 | 76 | 169 | 86 | 187 | 96 | 205
   57 | 135 | 67 | 152 | 77 | 170 | 87 | 188 | 97 | 207
   58 | 136 | 68 | 154 | 78 | 172 | 88 | 190 | 98 | 208
   59 | 139 | 69 | 158 | 79 | 174 | 89 | 192 | 99 | 210
   Alphanumeric Conversion Table
   Display Reading (Alphanumeric) | °C | °F | %
   --- | --- | --- | ---
   A1 thru A9 | −1 thru −9 | 30 thru 16 | −1 thru −9
   B0 thru B9 | −10 thru −19 | 14 thru −2 | −10 thru −19
   C0 thru C9 | −20 thru −29 | −4 thru −20 | −20 thru −29
   D0 thru D9 | −30 thru −39 | −22 thru −38 | −30 thru −39
   E0 thru E9 | −40 thru −49 | −40 thru −58 | ———
   F0 thru F9 | −50 thru −59 | −58 thru −74 | +100 thru +109