NOTE: Take care not to tear the seams or damage the seat covers. Put on gloves to protect your hands. Tilt the seat-back half-way forward, and tip the seat cushion up. Remove these items: Headrest and center headrest Cargo net (for some models) Seat-back top cover Armrest (right seat-back) Release the clips fastening the seat-back cover as needed, and unzip the cover. Right seat-back: Remove the center headrest guides from the seat-back. Recline the seat-back fully, and secure it. Pull out the seat belt (A) and center seat belt (B) (right seat-back) as needed, then pull out the seat-back cover/pad (C) from the frame (D). |