Remove the engine cover. Remove the drive belt. Remove the power steering (P/S) pump, and the P/S hose clamp. Do not disconnect the P/S hoses from the pump. Remove the alternator. Remove the A/C compressor. Do not disconnect the A/C line from the compressor. Remove the thermostat housing. Remove the oil filter housing assembly (A). Remove the oil filter assembly, engine oil cooler, drive belt auto-tensioner, and water pump, then replace the oil filter housing. Reassemble the oil filter housing reverse order of removal, then install the oil filter housing using the new O-rings (B). Install the thermostat housing. Install the A/C compressor. Install the alternator. Install the P/S pump and the P/S hose clamp. Install the drive belt. Install the engine cover. |