General Precautions Please read the following precautions carefully before performing the airbag system service. Observe the instructions described in this manual, or the airbags could accidentally deploy and cause damage or injuries. Except when performing electrical inspections, always turn the ignition switch OFF and disconnect the negative cable from the battery, and wait at least 3 minutes before beginning work. NOTE: The SRS memory is not erased even if the ignition switch is turned OFF or the battery cables are disconnected from the battery. Use replacement parts which are manufactured to the same standards and quality as the original parts. Do not install used SRS parts. Use only new parts when making SRS repairs. Carefully inspect any SRS part before you install it. Do not install any part that shows signs of being dropped or improperly handled, such as dents, cracks or deformation. Before removing any of the SRS parts (including the disconnection of the connectors), always disconnect the SRS connector. Use only a digital multimeter to check the system. If it is not a Honda multimeter, make sure its output is 10 mA (0.01 A) or less when switched to the lowest value in the ohmmeter range. A tester with a higher output could cause accidental deployment and possible injury. Do not put objects on the front passenger's airbag. The original radio has a coded theft protection circuit. Be sure to get the customer's radio code and write down the frequencies for the radio's preset stations before disconnecting the battery cable. Before returning the vehicle to the customer, enter the radio code, then enter the customer's radio station presets, the power window control unit reset procedure, and set the clock. Do the engine control module (ECM) idle learn procedure. After disconnecting the battery negative cable, do the power window control unit resetting procedure. |