Navigation Unit Inputs and Outputs for Connector E (2P)

Terminal Number | Wire Color | Terminal Name | Description | Voltage (about) | Symptom
--- | --- | --- | --- | --- | ---
1 | ——— | GPS | GPS signal (5 V in, GPS signal out) | 5 V | If open: GPS icon on screen is white, system links screen ANT shows ‘‘NG.'' If short to ground: Same as open.
2 | ——— | GND GPS | Ground for GPS signal | 0 V | If open: GPS icon on screen is white, system links screen ANT shows ‘‘NG.'' If short to ground: No effect on system.