Slide the steering gearbox (A) in the gearbox mounting bracket (B). Apply a neutral detergent (diluted with water) to the steering gearbox bushing (C) surfaces upper and lower. If you don't apply a neutral detergent to the bushing surfaces, the gearbox bushing will be damaged when installing the subframe. Loosely install the new subframe mounting bolts (D), stiffener mounting bolts (E), and new stiffener mounting bolts (F). |