Cruise Control Combination Switch Test/Replacement

SRS components are located in this area. Review the SRS component locations, for LHD models, for RHD models, and the precautions and procedures, before performing repairs or service. Remove the driver's airbag. Remove the two screws, then disconnect the connector, and remove the switch. |

Check for continuity between the terminals in each switch position according to the table. If there is continuity, and it matches the table, but switch failure occurred on the cruise control unit input test, check and repair the wire harness on the switch circuit. If there is no continuity in the appropriate positions, replace the switch. |