Regulator valve body spring

Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Wire Diameter | O.D. | Free Length | No. of Coil
Regulator valve body spring | Stator reaction spring |  | 4.5 mm (0.177 in.) | 35.4 mm (1.394 in.) | 30.3 mm (1.193 in.) | 1.92
Regulator valve spring A | K20Z2 engine model | 1.9 mm (0.075 in.) | 14.7 mm (0.579 in.) | 80.6 mm (3.173 in.) | 16.1
K24A3 engine model | 1.85 mm (0.073 in.) | 14.7 mm (0.579 in.) | 83.0 mm (3.268 in.) | 14.9
Regulator valve spring B |  | 1.6 mm (0.063 in.) | 9.2 mm (0.362 in.) | 44.0 mm (1.732 in.) | 12.5
Torque converter check valve spring |  | 1.2 mm (0.047 in.) | 8.6 mm (0.339 in.) | 33.8 mm (1.331 in.) | 12.2
Lock-up shift valve spring |  | 1.0 mm (0.039 in.) | 6.6 mm (0.260 in.) | 35.5 mm (1.398 in.) | 18.2
3rd accumulator spring |  | 2.5 mm (0.098 in.) | 14.6 mm (0.575 in.) | 29.9 mm (1.177 in.) | 4.9
1st accumulator spring A |  | 2.4 mm (0.094 in.) | 18.6 mm (0.732 in.) | 49.0 mm (1.929 in.) | 7.1
1st accumulator spring B |  | 2.3 mm (0.091 in.) | 12.2 mm (0.480 in.) | 31.5 mm (1.240 in.) | 6.6