Blower Unit Components Replacement

Note these items when overhauling the blower unit: The recirculation control motor (A), the blower motor (B), and the dust and pollen filter (C) can be replaced without removing the blower unit. Before reassembly, make sure that the recirculation control linkage and doors move smoothly without binding. After reassembly, make sure the recirculation control motor runs smoothly. NOTE: LHD type is shown, RHD type is symmetrical. |