EPS Control Unit Inputs and Outputs for Connector D (3P)

Terminal number | Wire color | Terminal sign (Terminal name) | Description | Measurement
--- | --- | --- | --- | ---
Terminals | Conditions (Ignition Switch ON (II)) | Voltage
1 | PNK | VS1 (voltage sensor 1) | Detects torque sensor signal | ——— | ——— | ———
2 | BLU/RED | PVF (Voltage fade) | Drives the torque sensor | ——— | ——— | ———
3 | WHT/GRN | VS2 (Voltage sensor 2) | Detects torque sensor signal | ——— | ——— | ———