Before testing the keyless entry/security control functions, troubleshoot the multiplex integrated control system. Multiplex Integrated Control Unit Remove the left kick panel (LHD type) or right kick panel (RHD type). Disconnect the under-dash fuse/relay box connectors. NOTE: All connectors are wire side of female terminals.
1. Inspect the connector and socket terminals to be sure they are all making good contact. If the terminals are bent, loose or corroded, repair them as necessary, and recheck the system. If the terminals look OK, go to Step 5 . With the connectors still disconnected, make these input tests at the connectors. If any test indicates a problem, find and correct the cause, then recheck the system. If the input tests prove OK, go to Step 6 .
   Cavity | Wire | Test condition | Test: Desired result | Possible cause if result is not obtained
   --- | --- | --- | --- | ---
   H9 | BLK | Under all conditions | Check for continuity to ground: There should be continuity. | Poor ground (G601) An open in the wire
   F5 | YEL/GRN | Connect the F5 terminal to the battery positive terminal momentarily. | Check trunk opener operation: Trunk lid should open. | Poor ground (G701) Faulty trunk opener solenoid An open in the wire
   K11 | YEL | Connect the battery positive terminal to K12 (K11) terminal, and K11 (K12) terminal to H9 terminal. | Check actuator operation: The driver's door lock actuator should lock (unlock). | Faulty driver's door lock actuator An open in the wire
   K12 | YEL/BLK
   N7 | YEL/BLK | Connect the battery positive terminal to N7 (N9) terminal, and N9 (N7) terminal to H9 terminal. | Check actuator operation: The front passenger's door lock actuator should lock (unlock). | Faulty front passenger's door lock actuator An open in the wire
   N9 | YEL
   E2 *1 H3 *2 | YEL/BLK | Connect the battery positive terminal to E2 or H3 (E8 or H10) terminal, and E8 or H10 (E2 or H3) terminal to H9 terminal. | Check actuator operation: The left rear door lock actuator should lock (unlock). | Faulty left rear door lock actuator An open in the wire
   E8 *1 H10 *2 | YEL
   H3 *1 E2 *2 | YEL/BLK | Connect the battery positive terminal to H3 or E2 (H10 or E8) terminal, and H10 or E8 (H3 or E2) terminal to H9 terminal. | Check actuator operation: The right rear door lock actuator should lock (unlock). | Faulty right rear door lock actuator An open in the wire
   H10 *1 E8 *2 | YEL
   P23 *1 P22 *2 | WHT *1 WHT/GRN *2 | Under all conditions | Check for continuity to ground: There should be continuity. | Faulty hazard warning light relay An open in the wire
   K2 *3 | LT GRN/RED | Under all conditions | Check for continuity between the K2 terminal and No. 1 terminal of the driver's actuator. There should be continuity. | An open in the wire
   E10 *3 | LT GRN/RED | Under all conditions | Check for continuity between the E10 terminal and No. 1 terminal of the right rear actuator. There should be continuity. | An open in the wire
   X13 *3 | GRY/RED | Under all conditions | Check for continuity between the X13 terminal and No. 6 terminal of the front passenger's or left rear actuator. There should be continuity. | An open in the wire
   *1: | LHD type
   *2: | RHD type
   *3: | With super locking
1. Reconnect all connectors to the under-dash fuse/relay box, and make these input tests at the appropriate connectors on the under-dash fuse/relay box. If any test indicates a problem, find and correct the cause, then recheck the system. If all the input tests prove OK, go to Step 7 .
   Cavity | Wire | Test condition | Test: Desired result | Possible cause if result is not obtained
   --- | --- | --- | --- | ---
   Q8 *1 Q13 *2 | BRN | Front passenger's door lock knob switch unlocked | Check for voltage to ground: There should be 1 V or less. | Poor ground (G503) Faulty front passenger's door lock knob switch An open in the wire
   Front passenger's door lock knob switch locked | Check for voltage to ground: There should be 5 V or more. | Faulty front passenger's door lock knob switch Short to ground
   Q2 *1 Q4 *2 | GRY *1 ·ORN *2 | Left rear door lock knob switch unlocked | Check for voltage to ground: There should be 1 V or less. | Poor ground (G501, G601) Faulty left rear door lock knob switch An open in the wire
   Left rear door lock knob switch locked | Check for voltage to ground: There should be 5 V or more. | Faulty left rear door lock knob switch Short to ground
   Q3 *1 Q5 *2 | WHT *1 ·RED *2 | Right rear door lock knob switch unlocked | Check for voltage to ground: There should be 1 V or less. | Poor ground (G602) Faulty right rear door lock knob switch An open in the wire
   Right rear door lock knob switch locked | Check for voltage to ground: There should be 5 V or more. | Faulty right rear door lock knob switch Short to ground
   Q8 *3 | YEL | Under all conditions | Check for continuity between the Q8 terminal and No. 2 terminal of the alarm control siren. There should be continuity. | An open in the wire
   *1: | LHD type
   *2: | RHD type
   *3: | With super locking
   Cavity | Wire | Test condition | Test: Desired result | Possible cause if result is not obtained
   --- | --- | --- | --- | ---
   Q1 *1 Q6 *2 | RED *1 ·RED/BLU *2 | Under all conditions | Check for continuity to ground: There should be continuity. | Poor ground (G504) Faulty connections at the audio unit Faulty audio unit An open in the wire
   P13 *1 P2 *2 | RED/WHT | Ignition key inserted into the ignition switch. | Check for voltage to ground: There should be 1 V or less. | Poor ground (G501, G601) Faulty ignition key switch An open in the wire
   Ignition key removed from the ignition switch. | Check for voltage to ground: There should be 5 V or more. | Faulty ignition key switch Short to ground
   E15 | GRN | Driver's door open | Check for voltage to ground: There should be 1 V or less. | Faulty driver's door switch An open in the wire
   Driver's door closed | Check for voltage to ground: There should be 5 V or more. | Faulty driver's door switch Short to ground
   H12 | LT GRN/RED | Front passenger's door open | Check for voltage to ground: There should be 1 V or less. | Faulty front passenger's door switch An open in the wire
   Front passenger's door closed | Check for voltage to ground: There should be 5 V or more. | Faulty front passenger's door switch Short to ground
   E14 *1 H13 *2 | GRN/YEL *1 GRN/WHT *2 | Left rear door open | Check for voltage to ground: There should be 1 V or less. | Faulty left rear door switch An open in the wire
   Left rear door closed | Check for voltage to ground: There should be 5 V or more. | Faulty left rear door switch Short to ground
   H13 *1 E14 *2 | GRN/WHT *1 GRN/YEL *2 | Right rear door open | Check for voltage to ground: There should be 1 V or less. | Faulty right rear door switch An open in the wire
   Right rear door closed | Check for voltage to ground: There should be 5 V or more. | Faulty right rear door switch Short to ground
   P24 *1 P21 *2 | PNK *1 LT GRN *2 | Trunk lid open | Check for voltage to ground: There should be 1 V or less. | Poor ground (G701) Faulty trunk latch switch An open in the wire
   Trunk lid closed | Check for voltage to ground: There should be 5 V or more. | Faulty trunk latch switch Short to ground
   P8 *1 P7 *2 | LT GRN *1 BLU *2 | Trunk opener switch pushed | Check for voltage to ground: There should be 1 V or less. | Poor ground (G701) Faulty trunk open switch An open in the wire
   Trunk opener switch released | Check for voltage to ground: There should be 5 V or more. | Faulty trunk open switch Short to ground
   *1: | LHD type
   *2: | RHD type