Radio Remote Switch Test - With Cruise Control

1. With cruise control ('05 model) Remove the driver's airbag assembly. Remove the 13P connector from the cable reel. Measure resistance between the No. 11 and No. 12 terminals in each switch position according to the table.
   Position | Resistance
   --- | ---
   OFF | About 10 kΩ
   MODE | About 6 kΩ
   CH (+) | About 2 kΩ
   CH (−) | About 840 Ω
   ▲ (VOL. UP) | About 370 Ω
   ▼ (VOL. DOWN) | About 100 Ω

Check the continuity between the No. 4 and No. 11 terminals in each switch position according to the table. If the resistance is not as specified, replace the remote switch. |