Remove the A/C condenser by lifting it up. Be careful not to damage the radiator and A/C condenser fins when removing the A/C condenser. Install the A/C condenser in the reverse order of removal, and note these items: If you're installing a new A/C condenser, add refrigerant oil (KEIHIN SP-10). Replace the O-rings with new ones at each fitting, and apply a thin coat of refrigerant oil before installing them. Be sure to use the correct O-rings for HFC-134a (R-134a) to avoid leakage. Immediately after using the oil, reinstall the cap on the container, and seal it to avoid moisture absorption. Do not spill the refrigerant oil on the vehicle; it may damage the paint; if the refrigerant oil contacts the paint, wash it off immediately. Be careful not to damage the radiator or the A/C condenser fins when installing the A/C condenser. Charge the system. Do the ECM/PCM idle learn procedure. Perform the power window control unit reset procedure. Enter the anti-theft codes for the radio and the navigation system, then enter the customer's radio station presets. |