Front Splash Shield Replacement

1. NOTE: Take care not to scratch the body. Remove the splash shield (A).
   -1. | From both wheel arch, remove the bolts (B), clips (C), and clip (D) (right side for some models) securing the front inner fender (E) and splash shield (on the body).
   -2. | From under the front bumper (F), remove the clips (C), and bolts (G) (with engine under cover).
   -3. | Release the hooks (H) of the splash shield, then pull the splash shield out.
Install the splash shield in the reverse order of removal, and note these items: Replace any damaged clips. Push the clips into place securely. |