ATF pump

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
ATF pump | ATF pump thrust clearance |  | 0.03−0.05 mm (0.001−0.002 in.) | 0.07 mm (0.003 in.)
ATF pump gear-to-body clearance | Drive gear | 0.210−0.265 mm (0.008−0.010 in.) | ———
Driven gear | 0.070−0.125 mm (0.003−0.005 in.) | ———
ATF pump driven gear I.D. |  | 14.016−14.034 mm (0.5518−0.5525 in.) | When worn or damaged
ATF pump driven gear shaft O.D. |  | 13.980−13.990 mm (0.5504−0.5508 in.) | When worn or damaged