How to Remove the ECM/PCM for Testing If DTC troubleshooting requires voltage or resistance checks at the ECM/PCM connectors, remove the ECM/PCM and test it: Jump the SCS line with the HDS. Remove the center lower covers (A). Remove the duct (B). Disconnect the ECM/PCM connectors (C). Remove the bolts (D), then remove the ECM/PCM (E). Install the ECM/PCM in the reverse order of removal. Open the SCS line with the HDS. |