1. Install the trim in the reverse order of removal, and note these items: Replace any damaged clips with new ones. If the side curtain airbag has deployed, replace the center pillar upper trim with a new one. To prevent the side curtain airbags from deploying improperly and possibly causing injury, inspect removed pieces and replace them if they have any of these types of damage:
   - | Any cracks or deformations in the center pillar upper trim (A) and the upper hooks (B), and any stress-whitenings in the upper part of the trim
   - | Any cracks or deformations in the center pillar lower trim (C), and any breakage in the part (D) that fits into the center pillar upper trim
   - | Any cracks or stress-whitening in the clip seating surfaces (E)
Replace any damaged parts with new ones. Make sure the top of the trim overlaps with the headliner correctly. Make sure the trim hooks are installed into the holes in the side curtain airbag center pillar bracket securely. Push the clips into place securely. Apply liquid thread lock to the front seat belt upper anchor bolt before reinstallation. Before installing the anchor bolt, make sure there are no twists or kinks in the seat belt. |