Installation Install the steering column in the reverse order of removal, and note these items: Make sure the wires are not caught or pinched by any parts. Take care not to let the sliding capsules fall out of position during column installation. Steering joint connection; center the steering rack within its stroke. Install the steering joint (A) aligning the slit (B) of the steering joint with the tab (C) of the center guide. Position the angle of center guide as shown if necessary. With the rack in the straight ahead driving position, cut the wire (D) and slip the lower end of the steering joint on to the pinion shaft (E). |