Maintenance Schedule - Except European Model
12,000miles(1year)

This Maintenance Schedule outlines the minimum required maintenance that you should perform to ensure the trouble-free operation of vehicle. Due to regional and climatic difference, some additional service may be required. Please consult the warranty booklet for a more detailed description.
About replacing engine oil, engine oil filter, manual transmission fluid (MTF) and automatic transmission (ATF)
Use the Normal Conditions schedule for replacing engine oil, engine oil filter, MTF and ATF, if the severe driving conditions specified in the severe driving conditions below do not apply, and if only OCCASIONALLY driving in severe driving conditions. If the vehicle is driven MAINLY in any of the following severe driving conditions, use the Severe Conditions schedule.
Severe Driving Conditions on engine oil and engine oil filter replacement:

- Driving less than 8 km (5 miles) per trip or, in freezing temperature, driving less than 16 km (10 miles) per trip.
- Driving in extremely hot over 35 °C (95 °F) conditions.
- Extensive idling, or long periods of stop-and-go driving
- Trailer towing, driving with a car-top carrier, or driving in mountains conditions.
- Driving on muddy, or de-iced roads.

Severe Driving Conditions on MTF and ATF replacement:

- Driving in extremely hot over 35 °C (95 °F) conditions.
- Trailer towing, driving with a car-top carrier, or driving in mountainous conditions.

Service at the indicated distance or time whichever comes first

| Replace engine oil filter

| Check parking brake adjustment
Check the parking brake operation

| Replace dust and pollen filter

Visually inspect the following items:
|  | Check for correct installation and position, check for cracks, deterioration, rust, and leaks
|  | Check tightness of screws, nuts, and joints. If necessary, retighten

| Brake hoses and lines (including ABS/VSA)
Check master cylinder, proportioning control valve, and ABS/VSA modulator control-unit and leakage

| All fluid level and check for leak
Check levels and check for leaks. If necessary.
|  | Engine coolant
|  | MTF
|  | ATF
|  | Brake fluid
|  | Windshield fluid

| Exhaust system
Check the exhaust pipe and muffler for damage, leaks, and tightness

| Fuel lines and connections
|  | Check fuel lines for loose connections, cracks, and deterioration
|  | Retighten loose connections and replace any damage parts

Every 10,000 km (6,250 miles) or 1 year

| Replace engine oil

Every 5,000 km (3,125 miles) or 6 months

| Replace engine oil

Every 10,000 km (6,250 miles) or 6 months

| Replace engine oil filter

| Inspect front and rear brakes
|  | Check the brake pad and disc thickness. Check for damage or cracks front pad , front disc , rear pad , rear disc
|  | Check the brake linings for cracking, grazing, wear, and contamination
|  | Check the calipers for damage, leaks, and tightness

Visually inspect the following items:

| Tie-rod ends, steering gearbox, and boots
Check rack grease and steering linkage. Check the boot for damage and leaking grease

| Suspension components
|  | Check the bolts for tightness
|  | Check all dust cover for deterioration and damage

| Driveshaft boots
|  | Check the boot and boot band for cracks
|  | Check rack grease

Every 10,000 km (6,250 miles)

| Clean air cleaner element (Dry type only)

| Rotate tyres
Check tyre inflation at least once per month

Every 20,000 km (12,500 miles)

| Replace air cleaner element

Every 40,000 km (25,500 miles)

| Inspect the valve clearance
Check the valve clearance

Every 80,000 km (50,000 miles) or 4 years If the fuel suspected to be contaminated with dust, every 40,000 km (25,000 miles) or 2 years

| Replace fuel filter

Every 40,000 km (25,000 miles)

| Replace spark plugs

Every 100,000 km (62,500 miles)

| Replace spark plugs

At 200,000 km (125,000 miles) or 10 years, thereafter every 100,000 km (60,000 miles) or 5 years

| Replace engine Coolant
Use genuine Honda Long Life Antifreeze/Coolant Type 2

Every 3 years

| Replace brake fluid
|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid
|  | Check that brake fluid level is between upper and lower marks on the reservoir