SRS Driver's Airbag Replacement

Removal Disconnect the battery negative cable and wait at least 3 minutes before beginning work. Remove the access panel (A) from the steering wheel, then disconnect the driver's airbag 2P connector (B) from the cable reel. |

Remove the two Torx bolts (A) using a Torx T30 bit. Disconnect the horn switch connector (1P), then remove the driver's airbag (B). |

Installation Connect the horn switch connector (1P) (A) to the driver's airbag. Place the new driver's airbag (B) in the steering wheel, and secure it with new Torx bolts (C). |

Connect the cable reel 2P connector (A) to the driver's airbag 2P connector, then install the access panel (B) on the steering wheel. Connect the battery negative cable. After installing the airbag, confirm proper system operation: Turn the ignition switch ON (II); the SRS indicator should come on for about 6 seconds and then go off. Make sure the horn works. |