Fuel Pump/Fuel Gauge Sending Unit Replacement

Relieve the fuel pressure. Remove the fuel fill cap. Fold the rear seat and rise the seat cushion. Remove the access panel (A) from the floor. Disconnect the fuel pump 5P connector (B). Disconnect the quick-connect fitting (C) from the fuel tank unit. |

Remove the fuel tank unit (A). |

Remove the fuel filter (A), the fuel gauge sending unit (B), and the wire harness (C). When connecting the fuel tank unit, make sure the connection is secure and the suction filter (D) is firmly connected to the fuel pump (E). Install the part in the revers order of removal with a new base gasket (F), then check these items: When connecting the wire harness, make sure the connection is secure and the connectors (G) are firmly locked into place. When installing the fuel gauge sending unit, make sure the connection is secure and the connector is firmly locked into place. Be careful not to bend or twist it excessively. When installing the grommet (H) and O-ring (I), coat the grommet with clean engine oil. |