If necessary, remove the clips (A) as shown, and disconnect the license light connectors (B), then remove the stiffener (C). Detach the clips (D), then remove the license light subharness (E) from the stiffener. Remove the clips (F), and license lights (G) from the trim (H). Install the trim in the reverse order of removal, and note these items: Make sure the license light connectors are plugged in properly. Replace any damaged clips with new ones. |