Front Subframe Alignment NOTE: Before removing the subframe, make reference marks on the subframe that line up with the edge of the rear bracket for reinstallation. When installing, align both installation reference holes in the subframe with the reference holes in the body using a screwdriver or tapered punch as a guide. After mounting the subframe and bracket loosely, align the reference marks with the edge of the rear bracket then tighten the bolts.