ECM Inputs and Outputs at Connector No. 1 (96P)
NOTE: Standard battery voltage is 12 V.

ECM Terminal number | Wire color | Terminal name | Description
--- | --- | --- | ---
57 | GRN/WHT | IMRCSG (SENSOR GROUND) | Sensor ground
60 | BLU | CMP (CAMSHAFT POSITION (CMP) SENSOR) | Detects CMP sensor signal
67 | RED/WHT | ECT (ENGINE COOLANT TEMPERATURE (ECT) SENSOR) | Detects ECT sensor signal
69 | BLK/WHT | MAFSG (SENSOR GROUND) | Sensor ground
70 | BLK | GCUGND (GLOW PLUG CONTROL MODULE GROUND) | Ground for glow plug control module
73 | BLU | INJ3− (No. 3 INJECTOR −SIDE) | Drives No. 3 injector
74 | BRN | INJ1− (No. 1 INJECTOR −SIDE) | Drives No. 1 injector
78 | WHT/BLK | T/CSOL (TURBOCHARGER BOOST CONTROL SOLENOID VALVE) | Drives turbocharger boost control solenoid valve
79 | RED/BLU | M-PROP (FUEL RAIL PRESSURE CONTROL VALVE) | Drives fuel rail pressure control valve
80 | WHT/GRN | ALTC (ALTERNATOR CONTROL) | Sends alternator control signal
81 | WHT/RED | IMRCS (INTAKE MANIFOLD RUNNER CONTROL (IMRC) SOLENOID VALVE) | Detects IMRC solenoid valve
84 | BLU/WHT | VSS (VEHICLE SPEED SENSOR (VSS)) | Detects VSS signal
86 | WHT | SEDIMENT (FUEL FILTER WATER LEVEL SWITCH) | Detects fuel filter water level switch
88 | BLU/RED | IAT1 (INTAKE AIR TEMPERATURE (IAT) SENSOR 1) | Detects IAT senor 1 (in the MAF sensor) signal
89 | GRN/RED | MAP (MANIFOLD ABSOLUTE PRESSURE (MAP) SENSOR) | Detects MAP sensor signal
90 | YEL | MAF (MASS AIR FLOW (MAF) SENSOR) | Detects MAF sensor signal
91 | GRN/YEL | RPSSG (SENSOR GROUND) | Sensor ground
92 | BLK | CKP+ (CRANKSHAFT POSITION (CKP) SENSOR +SIDE) | Detects CKP sensor
93 | WHT | CKP− (CRANKSHAFT POSITION (CKP) SENSOR −SIDE) | Detects CKP sensor
94 | LT GRN | CKPSHLD (CRANKSHAFT POSITION (CKP) SENSOR SHIELD) | Shield ground