Disconnect the dashboard wire harness 4P connector (A) from the cable reel. Connect the SRS inflator simulator (2 Ω connectors) and simulator lead F to the dashboard wire harness. Reconnect the battery negative cable. Erase the DTC memory. Read the DTC. Is DTC 11-3x indicated?
YES | - | Go to Step 15 .
NO | - | Short in the cable reel; replace the cable reel. ■
Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes. |