NOTE: Keep the oil pump chain away from magnetic fields. Removal Remove the drive belt. Remove the power steering (P/S) pump. Do not disconnect the P/S hoses from the pump. Install the engine hanger to the P/S pump bracket, then attach the chain hoist and support the engine. Remove the cam chain. Remove the oil pan. Loosely install the crankshaft pulley. To hold the rear balancer shaft, insert a 8 mm long pin punch (A) (Snap-on PPC110LA or equivalent) into the maintenance hole in the balancer shaft holder and through the rear balancer shaft. Turn the crankshaft counterclockwise to compress the oil pump chain auto-tensioner. |