A/C Receiver/Dryer Desiccant Replacement

Remove the A/C condensor. Remove the bolts from the A/C condenser, then remove the receiver/dryer (A), the bracket (B) and the O-rings (C). Install the receiver/dryer in the reverse order of removal, and note these items: Replace the O-rings with new ones, and apply a thin coat of refrigarent oil (KEIHIN SP-10) before installing them. Be sure to use the correct O-rings for HFC-134a (R-134a) to avoid leakage. |