With HID Lamp
Automatic headlights adjuster system is composed of the headlights adjuster control unit front and rear, headlights adjuster leveling sensors, and left and right headlight leveling motors.
The system detects the vehicle posture every three minutes during running constantly with the headlight switch ON, and after eight seconds when the vehicle is stopped running with the ignition switch ON (II) and headlight switch ON.
If the vehicle posture has been changed, adjust the headlight vertical position automatically.