EGR Cooler Replacement

Remove the engine cover. Drain the engine coolant. Remove the bolts, then move the expansion tank. NOTE: Do not disconnect the lines. Remove the nuts (A), and the EGR pipe (B). NOTE: When installing the EGR pipe, replace the gaskets (C). |

Disconnect the hose (A). Remove the bolts (B), and the EGR cooler (C). Install the sensor in the reverse order of removal with the new O-ring (D) and gasket (E), then refill the radiator with engine coolant. |